D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: A1 | Firmware Version: 1.10

| Setup | Advanced | Tools | Status | Support

- MENU
- Setup
- Advanced
- Tools
- Status

# sTATUS Help

- Device Info
- Log
- Stats
- Wireless

## Device Info

All of your Internet and network connection details are displayed on the Device Info page. The firmware version is also displayed here.

Note: Some browsers have limitations that make it impossible to update the WAN status display when the status changes. Some browsers require that you refresh the display to obtain updated status. Some browsers report an error condition when trying to obtain WAN status.

Depending on the type of WAN connection, you can take one of the following sets of actions:
LAN
Displays the LAN (Local Area Network) settings of your DIR-615.

WAN
DHCP Connection – Clicking the DHCP Release button unassigns the router's IP address. The router will not respond to IP messages from the WAN side until you click the DHCP Renew button or power-up the router again. Clicking the DHCP Renew button causes the router to request a new IP address from the ISP's server.
PPPoE, PPTP, L2TP Connection – Depending on whether the WAN connection is currently established, you can click either the Connect to attempt to establish the WAN connection or the Disconnect to break the WAN connection.
BigPond Connection – Depending on whether you are currently logged in to BigPond, you can click either the BigPond Login to attempt to establish the WAN connection or the BigPond Logout to break the WAN connection.
Wireless
This displays the SSID, Channel, and whether or not Encryption is enabled on the Wireless interface.

## Log

s

The DIR-615 keeps a running log of events and activities occurring on it at all times. The log will display up to 200 recent logs. Newer log activities will overwrite the older logs. You can save the log files or have them emailed to you by clicking on the Log Settings button . This is recommended as the logs are cleared every time the router is rebooted.
First Page - Click this button to go to the first page of the log.
Last Page - Click this button to go to the last page of the log.
Previous - Moves back one log page.
Next - Moves forward one log page.
Clear - Clears the logs completely.

## Stats

Displays all of the LAN, WAN, and Wireless packet transmit and receive statistics. Transmit –The number of packets sent from the router. Received –The number of packets received by the router.

## Wireless

Use this page in order to view how many wireless clients have associated with the DIR-615. This page shows the MAC address of each associated client, how long they have been associated, and the mode they are connecting in (802.11b, 802.11g, or draft 802.11n).

Copyright © 2004-2005 D-Link Systems, Inc.