D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / Advanced Wireless

Firmware Version: 1.01
Hardware Version: A1
Product Page: DIR-825

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Advanced Wireless

If you are not familiar with these Advanced Wireless settings, please read the help section before attempting to modify these settings.

Note: Only Administrator has access to these functionalities.

### Advanced Wireless Settings

Wireless Band : 2.4GHz Band

Transmit Power :

Beacon Period : (20..1000)

RTS Threshold : (0..2347)

Fragmentation Threshold : (256..2346)

DTIM Interval : (1..255)

802.11d Enable :

WLAN Partition :

Multicast To Unicast :

WMM Enable :

Aggregation Limit :

TPC Max Gain : (0..50)

Aggregation Max Size : (2000..65535)

Aggregation Num Packets : (1..64)

Force Short Slot for 11N Clients :

A-MPDU Aggregation :

Short GI :

Extra Wireless Protection :

WDS Enable :

WDS AP MAC Address : 0:

1:

2:

3:

4:

5:

(Leave blank or all 0's to disable WDS for that slot)

### Advanced Wireless Settings

Wireless Band : 5GHz Band

Transmit Power :

Beacon Period : (20..1000)

RTS Threshold : (0..2347)

Fragmentation Threshold : (256..2346)

DTIM Interval : (1..255)

802.11d Enable :

WLAN Partition :

Multicast To Unicast :

WMM Enable :

Aggregation Limit :

TPC Max Gain : (0..50)

Aggregation Max Size : (2000..65535)

Aggregation Num Packets : (1..64)

Force Short Slot for 11N Clients :

A-MPDU Aggregation :

Short GI :

Extra Wireless Protection :

WDS Enable :

WDS AP MAC Address : 0:

1:

2:

3:

4:

5:

(Leave blank or all 0's to disable WDS for that slot)

Helpful Hints...

It is recommended that you leave these parameters at their default values. Adjusting them could limit the performance of your wireless network.

Use 802.11d only for countries where it is required.

Enabling WMM can help control latency and jitter when transmitting multimedia content over a wireless connection.

More...

Copyright © 2004-2008 D-Link Systems, Inc.