dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup
- Logout

#
NETWORK SETUP

Select your connection type and enter the IP information if necessary.

## LAN SETTINGS

| DHCP Client |
| Static IP |
IP Address |
Subnet Mask |
Gateway IP Address |
DNS1 |
DNS2 |

##
PPPoE SETTINGS

PPPoE | Enable Disable
User Name | (e.g. name@isp.com)
Password |
Connection Status | Not Available.

##
DHCP SERVER SETTINGS

This section allows you to enable the built-in DHCP server to issue IP addresses to devices on your local network.

DHCP Server | Enable Disable
Starting IP Address |
Ending IP Address |
Lease Time |

## DHCP CLIENT LIST

Host Name | IP Address | MAC Address | Expired Time
DCS-3410 | 192.168.0.200 | 00:1e:58:b4:67:2a | 4days, 18 hours, 22 minutes, 38 seconds
| 192.168.0.201 | 00:24:36:16:cc:43 | expired
DCS-6410 | 192.168.0.202 | 00:03:1b:58:ef:3b | 1days, 6 hours, 11 minutes, 44 seconds
End_User | 192.168.0.203 | 00:1c:f0:78:d5:34 | 1days, 3 hours, 3 minutes, 7 seconds

Helpful Hints..
Points to remember while setting up a network connection:
- A static IP address is recommended for a network connection for easy management. The PPPoE connection is also useful for network setup.
- Any changes in the Network Settings will restart the system.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.