> > Port Mapping -- A maximum 16 entries can be configured

> > Port Mapping supports multiple port to PVC and bridging groups. Each group will perform as an independent network. To support this feature, you must create mapping groups with appropriate LAN and WAN interfaces using the Add button. The Remove button will remove the grouping and add the ungrouped interfaces to the Default group

> > Enable virtual ports on |

> > Group Name | Interfaces | Remove | Edit
> > Default | LAN(1-4), Wireless, Wireless_Guest |  |