D-LINK SYSTEMS, INC. | WIRELESS AP : HELP / Advanced

# Help MENU

Advanced

Advanced Wireless

Antenna Transmit Power - The antenna transmit power ranges from 12.5% (weak) to 100% (strong). The greater antenna transmit power, the longer the range of wireless communications. Select the power based on the coverage you desire for your DAP-1350. For security reasons, certain implementations require that the antenna transmit power be adjusted to provide wireless coverage within a limited area.
RTS threshold - This value should remain at its default setting of 2346. If you encounter inconsistent data flow, only minor modifications to the value range between 1 and 2347 are recommended. The default value for RTS Threshold is set to 2346.
Fragmentation threshold - This value should remain at its default setting of 2346. If you experience a high packet error rate, you may slightly increase your "Fragmentation" value within the value range of 256 to 2346. Setting the Fragmentation value too low may result in poor performance.

Copyright © 2009 D-Link Corporation/D-Link System, Inc.