D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: C1 | Firmware Version: 3.10NA |

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- VIRTUAL SERVER
- PORT FORWARDING
- APPLICATION RULES
- QOS Engine
- NETWORK FILTER
- ACCESS CONTROL
- WEBSITE FILTER
- INBOUND FILTER
- FIREWALL SETTINGS
- Routing
- ADVANCED WIRELESS
- ADVANCED NETWORK
- IPv6

# Advanced Wireless

If you are not familiar with these Advanced Wireless settings, please read the help section before attempting to modify these settings.

## Advanced Wireless Settings

Transmit Power : |
Beacon Period : | (20..1000)
RTS Threshold : | (0..2347)
Fragmentation : | (256..2346)
DTIM Interval : | (1..255)
WLAN Partition : |
WMM Enable : |
Short GI : |

Helpful Hints…

It is recommended that you leave these parameters at their default values. Adjusting them could limit the performance of your wireless network.

Use 802.11d only for countries where it is required.

Enabling WMM can help control latency and jitter when transmitting multimedia content over a wireless connection.

More…

Copyright © 2004-2008 D-Link Systems, Inc.