D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / Advanced Network

Firmware Version: 1.32NA
Hardware Version: A4
Product Page: DIR-655

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Advanced Network

If you are not familiar with these Advanced Network settings, please read the help section before attempting to modify these settings.

Note: Only Administrator has access to these functionalities.

### UPnP

Universal Plug and Play (UPnP) supports peer-to-peer Plug and Play functionality for network devices.

Enable UPnP :

Allow Users to disable Internet Access :

Allow Users to modify Virtual Server Mappings :

### WAN Ping

If you enable this feature, the WAN port of your router will respond to ping requests from the Internet that are sent to the WAN IP Address.

Enable WAN Ping Respond :

WAN Ping Inbound Filter :

Details :

### WAN Port Speed

WAN Port Speed :

### LAN Auto IP

Enable LAN Auto IP :

### Multicast Streams

Enable Multicast Streams :

Helpful Hints...

UPnP helps other UPnP LAN hosts interoperate with the router. Leave the UPnP option enabled as long as the LAN has other UPnP applications.

For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs.

The WAN speed is usually detected automatically. If you are having problems connecting to the WAN, try selecting the speed manually.

If you are having trouble receiving multicast streams from the Internet, make sure the Multicast Streams option is enabled.

More...

Copyright © 2004-2008 D-Link Systems, Inc.