dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- User Management
- RAID
- Backup and Restore
- Firmware Update
- Logout

#
BACKUP AND RESTORE

User can save the configurations to a file or restore it once necessary. Restart the NVR can keep system work freshly. Reset the NVR will restore all configuration to factory default.

##
BACKUP AND RESTORE

Save Configuration File |

Load Configuration File |

##
RESTART

System Restart |

##
DEFAULT

Restore to factory default settings. |  |
Set Configuration |  | IP |  | DDNS |

##
DEVICE SETTINGS

Name |

Helpful Hints..
Back and Restore: User can Save and backup configuration as a file to the specified location and restore it after reset to factory default. User also can restore the configuration file to another NVR.
Restart: If you found NVR not work properly or crash from some unknown reason, please restart NVR. Restart NVR will take about 1 and half minutes.
Reset to Default: This will reset all configurations to factory default. User can check the preserve functions from IP or DDNS, thus the remote connection will remain after reset.