dlink-ECEA07

Product Page: DNS-323 |  | Firmware Version: 1.09

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- WIZARD
- LAN
- DEVICE
- LOGOUT

# LAN SETTINGS :

The LAN Settings allows you to configure the Link Speed and to configure the IP address as a DHCP client or Static IP.

Enabling Jumbo Frames allows you to increase the Frame size from 3,000 to 9000 bytes which increase network throughput and performance. Standard Ethernet Frames are 1,500 bytes in size.

## LAN SETTINGS :

| Speed 100 Mbps
| Link Speed Auto 100 1000

| DHCP Client
| Static IP
| IP Address : |
| Subnet Mask : |
| Gateway : |
| DNS1 : |
| DNS2 : |

## JUMBO FRAME SETTINGS :

| Status : | Enable Disable
| MTU : |

Helpful Hints..
A Static IP is recommended if you will be using the FTP server.

Copyright © 2006-2009 D-Link Corporation/D-Link Systems, Inc.