> > ADSL Statistics

> > Mode: | N/A
> > Type: | N/A
> > Line Coding: | N/A
> > Status: | Link Down
> > Link Power State: | L0
> > | Downstream | Upstream
> > SNR Margin (dB): | N/A | N/A
> > Attenuation (dB): | N/A | N/A
> > Output Power (dBm): | N/A | N/A
> > Attainable Rate (Kbps): | N/A | N/A
> > Rate (Kbps): |  |
> > K (number of bytes in DMT frame): | N/A | N/A
> > R (number of check bytes in RS code word): | N/A | N/A
> > S (RS code word size in DMT frame): | N/A | N/A
> > D (interleaver depth): | N/A | N/A
> > Delay (msec): | N/A | N/A
> > Super Frames: | N/A | N/A
> > Super Frame Errors: | N/A | N/A
> > RS Words: | N/A | N/A
> > RS Correctable Errors: | N/A | N/A
> > RS Uncorrectable Errors: | N/A | N/A
> > HEC Errors: | N/A | N/A
> > OCD Errors: | N/A | N/A
> > LCD Errors: | N/A | N/A
> > Total Cells: | N/A | N/A
> > Data Cells: | N/A | N/A
> > Bit Errors: | N/A | N/A
> > Total ES: | N/A | N/A
> > Total SES: | N/A | N/A
> > Total UAS: | N/A | N/A