D-Link Corporation. | WIRELESS INTERNET CAMERA | SETUP | FTP

Product: DCS-920 |  | Firmware Version: 1.00

| Live Video | Setup | Maintenance | Status | Help

Wizard
Network Setup
Wireless Setup
Dynamic DNS
Image Setup
Video
Mail
FTP
Time and Date
Logout

# FTP

In this section, you may configure a FTP server to receive the images.

## FTP Server

Host Name |
Port | (Default is 21)
User Name |
Password |
Path |
Passive Mode | Yes No

## Time Schedule

| Enable uploading images to the FTP server

Always

| Schedule
| Day | Mon Tue Wed Thu Fri Sat Sun
| Time Period | Start : (Example : 06:30:00) Stop : (Example : 22:30:00)

Video Frequency |  |  | Frames/Second
|  | Seconds/Frame
Base File Name |
File | Overwrite
Date/Time Suffix
Sequence Number Suffix Up to

## Test FTP Server

| A JPEG file will be sent to the above FTP server for testing. (File name: test_date_time.jpg) |

Helpful Hints..
Host Name:
This is the IP address of the FTP server that you will be connecting to.
Port:
The default port is 21.
User Name:
The user name that required accessing the external FTP server.
Password:
The password of the external FTP server.
Passive mode - Enabling passive mode will allow access to an external FTP server if your camera is behind a router protected by a firewall.
Enable uploading images to the FTP server:
Checking this box will enable the camera to upload images to above FTP server.
Select Always to enable camera uploading images to the FTP server always.
Select Schedule if you like to specify the time and day when the camera to start and stop uploading the images to the FTP server.
Video Frequency - User can choose and define the numbers for both Frames/Second and Seconds/ Frame.
Base File Name - The name that contains the time stamp information, for example DCS-920
_2005072116425101.jpg. This means that the camera took a snapshot in the year 2005, July 21 at 16:42:51 (hour:min:sec) and 01 represents the 1st picture.
File - Select Overwrite and there will be only one images that are constantly refreshed . Select Date/Time Suffix and the pictures will be named with a date and time (may refer to Base File Name). An example of this can be seen under the Base file name category. Select Sequence Number Suffix up to 1024 and all the pictures will be numbered from 1-1024. The total amount of pictures can be configured up to 1024 pictures.
Test FTP server
An image file will be sent to the FTP server after you have clicked Test.

Copyright (C) 2007-2008 D-Link Corporation.