> > WAN
> > WAN IP Settings
> > Enter information provided to you by your ISP to configure the WAN IP settings. Notice: DHCP can be enabled for PVC in MER mode or IP over Ethernet as WAN interface if "Obtain an IP address automatically" is chosen.Changing the default gateway or the DNS effects the whole system. Configuring them with static values will disable the automatic assignment from DHCP or other WAN connection.
> > If you configure static default gateway over this PVC in MER mode, you must enter the IP address of the remote gateway in the "Use IP address".

> > Obtain an IP address automatically
> > Use the following IP address:
> > WAN IP Address: |
> > WAN Subnet Mask: |

> > Obtain default gateway automatically
> > Use the following default gateway:
> > | Use IP Address: |

> > Obtain DNS server addresses automatically
> > Use the following DNS server addresses:
> > | Primary DNS server: |
> > | Secondary DNS server: |