> > DNS Server Configuration

> > If 'Enable Automatic Assigned DNS' checkbox is selected, this router will accept the first received DNS assignment from one of the PPPoA, PPPoE or MER/DHCP enabled PVC(s) during the connection establishment. If the checkbox is not selected, enter the primary and optional secondary DNS server IP addresses. Click 'Apply' button to save the new configuration. You must reboot the router to make the new configuration effective.

> > | Enable Automatic Assigned DNS

> > Primary DNS server: |
> > Secondary DNS server: |