UPnP
Virtual Server
Lan Clients
SNMP
Filters
Bridge Filters
Routing
DMZ
Firewall
RIP
PPP
ADSL
ATM VCC
Wireless Management
Wireless Performance
Logout

Wireless Performance
These are the Wireless Performance feature for the AP(Access Point) portion.
Beacon interval: | (msec, range:1~1000,default:200)
DTIM: | (range:1~25,default:2)
Hidden SSID: | Enabled
Antenna transmit power: |
RTS Threshold: |
Frag Threshold: |
b/g Mode: |