Maintenance

Server is restarting now. It will automatically reconnect to http://ip_address:port/ after 55 seconds. If it has failed to make a connection, you must reconnect to the server manually by entering the IP address in the URL field in your browser.

Maintenance

Reboot system
Reboot the system. |
Factory default
Restore factory settings and lose any changes? System will restart and need installer program to setup network. |
Calibrate
Recalibrate the home position to the default center to recover the tolerance caused by some external forces. |
Upgrade firmware
Select firmware file: and click |