dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Menu
- Live Video
- Playback
- Setup
- Maintenance
- Status
- Logout

#
HELP MENU

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup

##

The Wizard is an easy to use utility for basic setup of the NVR. Here you can configure the administrator's password, time zone, LAN connection type, and additional settings of your NVR.

Step 1: Click Run Wizard to begin.
Step 2: Click Next to this introductory screen.
Step 3: Set Password - Enter the new administrator's password here. Enter it a second time for verification. Click Next.
Step 4: Choose Time Zone Choose your time zone from the drop down list. Click Next.
Step 5: Select LAN Connection Type - Choose DHCP Client or Static IP. DHCP Client should be selected if there is a DHCP server onthe network. Static IP should be selected when a DHCP server is not on the network. If you select Static IP, enter the required information.
Step 6: Set Additional Information - Enter device namehere. If you do not need to change this, you can leave the default entries in place. Click Next.
Step 7: Click Restart to save your settings and reboot the system

##

DHCP
Select this connection if you have a DHCP server running on your network and would like a dynamic IP address to be updated to your camera automatically.
Static IP
You may obtain a static or fixed IP address and other network information from your network administrator for your camera. A static IP address will ease you for accessing your camera in the future.
IP Address
The fixed IP address.
Subnet Mask
The default value is "255.255.255.0." Used to determine if the destination is in the same subnet.
Gateway IP Address
The gateway used to forward frames to destinations in a different subnet. Invalid gateway settings may cause the failure of transmissions to a different subnet.
DNS1
Primary domain name server that translates names to IP addresses.
DNS2
Secondary domain name server to backup the primary one.
PPPoE(Point-to-Point Protocol over Ethernet)
If you use the device to connect directly to the Internet you will need to put in the username and password that was given to you when you set up your account with the Internet Service Provider in these fields.
DHCP SERVER
The DHCP server can be used to serve IP addresses to devices on a network. Do not use this feature if you already have a DHCP server, such as a router, on the network.
DHCP Server
Enable or disable the DHCP server.
Starting IP Address
Enter the first IP address you would like to distribute on the network.
Ending IP Address
Enter the last IP address you would like to distribute on the network.
Lease Time
The duration of time that an IP address will remain assigned to a device. After this time expires, a new IP address will be given.
The DHCP Client List will show all devices that are receiving DHCP from the DNS-722-4.

##

Step 1: Click the Search button to search UPnP cameras. The system will list all the available cameras at this moment. Click the icon "+" to add this camera into your camera list.
Step 2: After clicking the icon , the camera setting page will pop-up. Click the item which you want to add a camera.
Step 3: Input the camera name, user name, and password of the camera.

Note
- Some cameras will limit the login authority to the administrator only.
- To add cameras without the UPnP function, please go to Camera Setup menu and enter the IP address manually.
-You may not be able to see all the cameras on your first search. It takes time for the devices to respond to UPnP request. Please click Search again.

Step 4: Click the Add button to add it.
Step 5: After clicking the Add button, the updated camera list will be displayed in the Camera list.
Step 6: Repeat step 2 through 5 to add other cameras in your list.

##

Step 1: Click the camera which you want to modify.
Step 2: Modify its information on the top of the page.
Step 3: Click the Save Settings button.
Step 4: If you want to replace a camera, click that camera, modify its address, port, user name, and password, and then click the Save Settings button.

Camera Channel
Select the number of analog cameras supported by one video server from the list.

Vendor
Displays the manufacturer's name.

Auto Detection
If you already input the camera IP and then you can simply click to automatically detect all the information (such as camera channel, protocol used, vendor, model number) of the camera.

Note Some cameras will limit the login authority to the administrator only.

##

Step 1: Click the camera which you want to modify in the camera list.
Step 2: NVR will get the parameter from camera, and you can modify its information at this page.
Camera Name
The name of this camera.
Video Format
Select the format which this camera supports.
Frame rate
Choose the frame rate.
Resolution
Choose the resolution.
Quality
Choose the image quality.
Audio
Check the Enable Audio option for live view and recording.
Go to Web
Allow user connects to the web page of network camera for advance setup. For example, the motion detection you should setup in the camera web interface first to enable NVR receive the trigger message.
Step 3: Click the Save Settings button.

Note The system will adjust the frame rate automatically based on the maximum frame rate which that camera can support.

##

Live Streaming Server
Port
Live streaming transmission port.
Maximum Connections
Maximum connections from remote access. The maximum number of remote connections is 32.
Playback Server Port Playback transmission port.
Maximum Users The number of users who can access playback functions at the same time. The maximum number of users for the playback server is 8.
Blocked/ Allowed List Allowed List: IP addresses in this list can log in Blocked List: IP addresses in this list will always be blocked

Note When setting Maximum Connections in Live Streaming Server settings, 1 connection means that 1 user can connect to 1 camera only. If the maximum number of connections is 16 and if a user connects to 4 cameras, the number of connected users is 4 and not 16.

##

Set Recording Mode
No Record
Turn off the recording.
Record by Schedule
Recording by schedule.
Always Record
Turn on the chosen cameras to record always.
Automatic Overwrite
Select this option to automatically empty disk space when the disk space is full. This will overwrite the earliest recorded video with the latest video one day at a time.
Store Videos by Schedule
Set duration to store recorded video clips. After this, the clips will be purged and cannot be recovered.
Set Recording Schedule
Day
Schedule the cameras to turn the recorder on and off at the same time every day according to your setting.
Week
Schedule the cameras for each day of the week differently.
Setup the Schedule
Step 1: Click the schedule of the camera which needs to be modified.
Step 2: Click the column on the bottom of the page.
Step 3: The default setting of the camera's recording schedule is from 00:00 to 24:00. If you want to modify the time slot, click the Configure button to modify the default settings first.
Insert
Insert new schedules.
Delete
Delete the selected schedule.
Configure
Modify the schedule and recording mode setting.Set Recording Schedule Configuration
Step 1: Setup the recording period
Step 2: Setup pre-record period and Post-record for event trigger recording.
Step 3: Choose the recording mode and the trigger source.
Step 4: Press OK to add this new schedule.
Step 5: If you want to add another new schedule, click the Insert button to add a new one.

Notes
- The Always Record option will start recording immediately.
- When configuring the Motion Detection event, ensure to setup the motion detection function in your camera first.
- When changing the motion detection settings of your camera, ensure to disconnect the NVR and then re-connect to update the settings in your NVR.
- When setting up an event, a video motion or digital input can be used to trigger the other cameras. This means that when motion is detected by a camera, it can send out warning signals to the other connected cameras.
- An alternative option is to drag the time bar to change the recording time period. The red bar represents the"Always Record" feature and the blue bar represents the "Event Recording" feature.

##

Step 1: Choose the camera, and then select one of the events.
Step 2: Click the Add button, and then click Email. Last, select the corresponded email addresses for contact person and click OK
Hence, if the event happens, the system will send an E-Mail to the pre-set contacts.
Step 3 Repeat steps 1 through 2 to set more cameras.
Note: You may select the Configure button to enable and schedule the event period for Camera List. Likewise, you may select the other Configure button to modify the contact.

##

Server Address
SMTP (Simple Mail Transport Protocol) server IP address.
Sender
Sender information.
Subject
The E-mail subject.
Body of Message
The E-Mail content.
SMTP Authentication
Provide the user name and password to the SMTP server for identification before sending E-Mail.
User Name
Input the SMTP server login user name.
Password
Input the SMTP server login user password.
Add Event Contacts
Step 1: Insert the name of a new contact.
Step 2: Insert the E-Mail of this new contact.
Step 3: Click the Add Contact button.
Step 4: Click the Save Settings button to save this modification of the contact list.

##

Enable this option only if you have purchased your own domain name and registered with a dynamic DNS service provider. The following parameters are displayed when the option is enabled.
Server Address
Select a dynamic DNS service provider from the pull-down list.
Host Name
Enter your host name, fully qualified; for example: myhost.mydomain.net.
Username or Key
Enter the username or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Password or Key
Enter the password or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Verify Password or Key
Re-type the password or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Status
Displays the current status of connection to DDNS server.

##

Time Zone Settings
Select your time zone from the pull-down list. Click Set Time to apply the settings.
There are three choices for setting the time.
NTP Server
Select or enter an NTP Server here. An NTP Server is a server on the Internet that maintains time. The NVR will contact the server you entered and receive the correct time. Click Set Time after entering an NTP Server.
From My Computer
Click Set Time to have the NVR set its own clock according to the time on your computer.
Manually Set The Time And Date
Enter the complete time and date settings manually. Click Set Time to apply the settings.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.