D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / Virtual Server

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Virtual Server

The Virtual Server option allows you to define a single public port on your router for redirection to an internal LAN IP Address and Private LAN port if required. This feature is useful for hosting online services such as FTP or Web Servers.

Note: Only Administrator has access to some of these functionalities.

### 8--VIRTUAL SERVERS LIST

|  |  | Port | Traffic Type
--- | --- | --- | --- | ---
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |
| Name |  | Public | Protocol
IP Address |  | Private |

Helpful Hints...

Check the Application Name drop down menu for a list of predefined server types. If you select one of the predefined server types, click the arrow button next to the drop down menu to fill out the corresponding field.

You can select a computer from the list of DHCP clients in the Computer Name drop down menu, or you can manually enter the IP address of the computer at which you would like to open the specified port.

More...

Copyright © 2009 D-Link Corporation/D-Link System, Inc.