dlink-B4938F

Product Page: DNS-343 |  | Firmware Version: 1.03

| Setup | Advanced | Maintenance | Status | Support

- Admin Password
- System
- Firmware Upgrade
- Email Alerts
- Power Management
- Dynamic DNS
- OLED Display
- Disk Diagnostic
- Logout

# E-MAIL ALERTS :

This section allows you to configure e-mails to be alerting you to certain operational conditions and drive status conditions. These alerts can prove helpful with the management and safeguarding of important data.

## E-MAIL ALERT SETTINGS :

| Login Method : | Account Anonymous
| User Name : |
| Password : |
| SMTP Server : |
| Sender E-mail : |
| Receiver E-mail : |

## ALERT TYPES :

Space Status Interval: (Hours) (Minutes)
One Of The Volumes Is Full
One Of The Hard Drives Has Failed
A Volume is degraded A Volume is rebuilt completed
The Administrator Password Has Been Changed
Firmware Has Been Upgraded
Send log file

Time: : | Day of week: Day of month:

Send S.M.A.R.T. Test Result
System Temperature Has Exceeded
Enabling this feature will cause the DNS-343 to shut down after the selected temperature is exceeded and an e-mail is sent.

Helpful Hints..
The SMTP server is your outgoing mail server. If you aren't sure what this is, contact the company that provides e-mail services for you.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.