D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Internet Setup
- Wireless Setup
- Network Setup
- LCD Setup

# Network Setting

Use this section to configure the internal network settings of your router and also to configure the built-in DHCP server to assign IP addresses to computers on your network. The IP address that is configured here is the IP address that you use to access the Web-based management interface. If you change the IP address in this section, you may need to adjust your PC's network settings to access the network again.

Please note that this section is optional and you do not need to change any of the settings here to get your network up and running.

## Router Settings

Use this section to configure the internal network settings of your router. The IP address that is configured here is the IP address that you use to access the Web-based management interface. If you change the IP address here, you may need to adjust your PC's network settings to access the network again.

Router IP Address : |
Default Subnet Mask : |
Local Domain Name : |
Enable DNS Relay : |

## DHCP Server Settings

Use this section to configure the built-in DHCP server to assign IP address to the computers on your network.

Enable DHCP Server : |
DHCP IP Address Range : | to (addresses within the LAN subnet)
DHCP Lease Time : | (minutes)

## DHCP Client List

Host Name | IP Address | MAC Address | Expired Time |
End_User | 192.168.0.100 | 00:04:23:2C:44:9F | 13 hr(s) 38 min(s)

## 25 - DHCP Reservation

Remaining number of clients that can be configured : 25

| Computer Name | IP Address | MAC Address |

Helpful Hints..
• If you already have a DHCP server on your network or are using static IP addresses on all the devices on your network, uncheck Enable DHCP Server to disable this feature.

More...

Copyright © 2004-2007 D-Link Systems, Inc.