D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / WISH

Firmware Version: 1.01
Hardware Version: A1
Product Page: DIR-825

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## WISH

WISH (Wireless Intelligent Stream Handling) prioritizes the traffic of various wireless applications.

Note: Only Administrator has access to these functionalities.

### WISH

Enable WISH :

### Priority Classifiers

HTTP :

Windows Media Center :

Automatic : (default if not matched by anything else)

### 24 -- WISH Rules

| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to
| Name | Priority | Protocol <<
Host 1 IP Range to | Host 1 Port Range to
Host 2 IP Range to | Host 2 Port Range to

Helpful Hints...

Enable this option if you want to allow WISH to prioritize wireless traffic.

For most applications, the priority classifiers ensure the right priorities, and specific WISH Rules are not required.

More...

Copyright © 2004-2008 D-Link Systems, Inc.