Network

Server is restarting now. It will automatically reconnect to http://ip_address:port/ after 55 seconds. If it has failed to make a connection, you must reconnect to the server manually by entering the IP address in the URL field in your browser.

Network settings

General
| LAN
| Get IP address automatically
| Use fixed IP address
| IP address |
| Subnet mask |
| Default router |
| Primary DNS |
| Secondary DNS |
| Enable UPnP
| Enable UPnP port forwarding
| PPPoE
| User name |
| Password |
| Confirm password |
HTTP
| HTTP port |
RTSP streaming
| Enable RTSP authentication
| Access name |
| RTSP port |
| RTP port for video |
| RTCP port for video |
| RTP port for audio |
| RTCP port for audio |
Note: RTP video port and RTP audio port must be an "even" number. RTCP video port and RTCP audio port must be RTP video port and RTP audio port add "1" individually.

WLAN configuration
| Disable WLAN
| SSID |
| Wireless mode |
| Channel |
| TX rate |
| Security |

| Algorithm |
| Pre-shared key |

| Auth mode |
| Key length |
| Key format |

| Default key | Network key
| 1 |
| 2 |
| 3 |
| 4 |