D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Website Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- Guest Zone
- Wake on LAN

# Guest Zone

Use this section to configure the guest zone settings of your router. The guest zone provides a separate network zone for guests to access the Internet.

## Guest Zone Selection

Enable Guest Zone : |
Wireless Network Name : | (Also called the SSID)
Security Mode : |

## WEP

WEP is the wireless encryption standard. To use it you must enter the same key(s) into the router and the wireless stations. For 64 bit keys you must enter 10 hex digits into each key box. For 128 bit keys you must enter 26 hex digits into each key box. A hex digit is either a number from 0 to 9 or a letter from A to F. For the most secure use of WEP set the authentication type to "Shared Key" when WEP is enabled.

You may also enter any text string into a WEP key box, in which case it will be converted into a hexadecimal key using the ASCII values of the characters. A maximum of 5 text characters can be entered for 64 bit keys, and a maximum of 13 characters for 128 bit keys.

Authentication | :
WEP Encryption | :
Default WEP Key | :

WEP Key | : (5 ASCII or 10 HEX)

WEP Key | : (13 ASCII or 26 HEX)

## WPA Only

WPA Only requires stations to use high grade encryption and authentication.

## WPA2 Only

WPA2 Only requires stations to use high grade encryption and authentication.

## WPA/WPA2

WPA/WPA2 requires stations to use high grade encryption and authentication.

Cipher Type | :
PSK / EAP | :

Network Key | : (8~63 ASCII or 64 HEX)

802.1X

RADIUS Server | IP Address | :
| Port | :
| Shared Secret | :

## Router Setting for the Guest Zone

Use this section to configure the guest zone settings of your router. The guest zone provides a separate network zone for guests to access the Internet.

Router IP Address : |
Default Subnet Mask : |

## Guest Zone Client Isolation

Enable the function to prevent guest clients accessing other guest clients in the Guest Zone. Guest clients can only access the Internet.

Enable Guest Zone Client Isolation : |

## Routing Between Host Zone And Guest Zone

Use this section to enable routing between the Host Zone and Guest Zone, Guest clients can not access Host clients' data without enabling this function.

Enable Routing Between Zones : |

## DHCP Server Settings For Guest Zone

Use this section to configure the built-in DHCP server to assign IP addresses to computers on your network.

Enable DHCP Server : |
DHCP IP Address Range : | to (addresses within the LAN subnet)
DHCP Lease Time : | (minutes)

## DHCP Client List For Guest Zone

Host Name | IP Address | MAC Address | Expired Time |

## Locked Client List For Guest Zone

The function is used to lock all PC clients which are in the Guest Zone to an IP/MAC address bundle list; only PCs in this list can access the network after enabling the function. This makes sure that no additional clients can access the Guest Zone regardless of whether they are using a wired or wireless connection.

Enable LOCK CLIENT LIST : |

Helpful Hints...

• Use this section to configure the guest zone settings of your router. The guest zone provide a separate network zone for guests to access Internet.

More...

Copyright © 2004-2007 D-Link Systems, Inc.