D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-600 | Hardware Version: A1 | Firmware Version : 1.01NA |

| Setup | Advanced | Tools | Status | Support

- Virtual Server
- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Access Control
- Website Filter
- Inbound Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- IPv6

# Advanced Network

If you are not familiar with these Advanced Network settings, please read the help section before attempting to modify these settings.

## UPnP

Universal Plug and Play (UPnP) supports peer-to-peer Plug and Play functionality for network devices.

Enable UPnP : |

## WAN Ping

If you enable this feature, the WAN port of your router will respond to ping requests from the Internet that are sent to the WAN IP Address.

Enable WAN Ping Respond : |
WAN Ping Inbound Filter : |
Details : |

## WAN Port Speed

WAN Port Speed : |

## Multicast Streams

Enable Multicast Streams : |

Helpful Hints…

UPnP helps other UPnP LAN hosts interoperate with the router. Leave the UPnP option enabled as long as the LAN has other UPnP applications.

For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs.

The WAN speed is usually detected automatically. If you are having problems connecting to the WAN, try selecting the speed manually.

If you are having trouble receiving multicast streams from the Internet, make sure the Multicast Streams option is enabled.

More…

Copyright © 2004-2009 DLink, Inc.