D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / DMZ

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## DMZ Settings

The DMZ (Demilitarized Zone) option lets you set a single computer on your network outside of the router. If you have a computer that cannot run Internet applications successfully from behind the router, then you can place the computer into the DMZ for unrestricted Internet access.

Note: Putting a computer in the DMZ may expose that computer to a variety of security risks. Use of this option is only recommended as a last resort.

Note: Only Administrator has access to some of these functionalities.

### DMZ Host

Enable DMZ :

DMZ IP Address :

Helpful Hints...

Enable the DMZ option only as a last resort. If you are having trouble using an application from a computer behind the router, first try opening ports associated with the application in the Virtual Server sections.

More...

Copyright © 2009 D-Link Corporation/D-Link System, Inc.