D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / Firewall Settings

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Firewall Settings

The Firewall Settings allow you to set a single computer on your network outside of the router.

Note: Only Administrator has access to some of these functionalities.

### Firewall Settings

Enable SPI :

### NAT Endpoint Filtering

Endpoint Independent

UDP Endpoint Filtering: Address Restricted

Port And Address Restricted

Endpoint Independent

TCP Endpoint Filtering: Address Restricted

Port And Address Restricted

### Anti-Spoof checking

Enable anti-spoof checking :

Helpful Hints...

ALGs provide special handling of the IP payload for some protocols and applications to make them work with network address translation (NAT).

More...

Copyright © 2009 D-Link Corporation/D-Link System, Inc.