DSL-G604T

Tools
Administrator Settings There are only one account that can access the DSL-G604T's Web-Management interface. It is admin. Admin has read/write access privilege. In this web page, you can set new password for admin.
Time The system time is the time used by the DSL-G604T for scheduling services. You can manually set the time or connect to a NTP (Network Time Protocol) server. If an NTP server is set, you will need to set the time zone, you may also set Daylight Saving dates and the system time will automatically adjust on those dates.
Remote Log Remote Log Server collects the logs sent from our device withcorrect log level.Users can setup the remote log server ip and the log level of our device.Then administrators are able to know the events happened on our device.

System Settings
The current system settings can be saved as a file onto the local hard drive. The saved file or any other saved setting file can be loaded back on the DSL-G604T. To reload a system settings file, click on Browse to browse the local hard drive and locate the system file to be used. You may also reset the DSL-G604T back to factory settings by clicking on Restore.
Save and Reboot - Settings need to be saved to Flash and the system needs to be rebooted for changes to take effect.
Restore - Use this button to restore factory default configuraion.NOTE:Connectivity to the unit will be lost.You can reconnect after the unit reboots.
Restart AP - Use this button to restart the Wireless Access Point.It is important to Restart Access Point any time you change your Wireless settings.

Firmware Upgrade You can upgrade the firmware of the DSL-G604T in this page. Make sure the firmware you want to use is on the local hard drive of the computer. Click on Browse to browse the local hard drive and locate the firmware to be used for the update.

Miscellaneous Item
These are additional tools and features of the DSL-G604T.
Ping Test - This useful diagnostic utility can be used to check if a computer is on the internet. It sends ping packets and listens for replies from the specific host.
IGMP Proxy - Here is the global setting for IGMP Proxy. If it is enabled, then the enabled IGMP Porxy on WAN PVCs will be working. Otherwise, no WAN PVC can have IGMP Proxy working on it.

Test The Diagnostic Test page shows the test results for the connectivity of the physical layer and protocol layer for both LAN and WAN sides.