D-LINK SYSTEMS, INC. | WIRELESS AP : ADVANCED / ACCESS CONTROL

Product Page: DAP-1360 | Firmware Version: V1.01

| SETUP | ADVANCED | MAINTENANCE | STATUS | HELP

- ADVANCED WIRELESS
- ACCESS CONTROL
- USER LIMIT
- LOGOUT

# Access Control :

The DAP-1360 can be setup to deny or only allow access to wireless clients with the listed MAC addresses.

## Wireless Access Settings

Use the client's MAC Address to authorize network access through the Access Point.

Access Control : |
MAC Address : | : : : : :
Connected PCs : |

## MAC Filter List

MAC Address | Edit | Del |

## IP Filter Rules

Entries in this table are used to restrict certain types of data packets from your local network to Internet through the Gateway. Use of such filters can be helpful in securing or restricting your local network.

|  |  | Traffic Type | Comment
| IP Address |  |  |

## IP Filter List

Current IP Filter Table:

Local IP Address | Protocol | Comment | Select

Helpful Hints..
Wireless Access Settings:
Create a list of MAC addresses that you would either like to accept or reject access to your network.
Connected PCs:
It will show the MAC address of all connected STAs. You can select what you want and click "clone". Then the MAC address will show into "MAC address" part automatically.
IP Filter:
Entries in this table are used to restrict certain types of data packets from your local network to Internet through the Gateway. Use of such filters can be helpful in securing or restricting your local network.

Copyright © 2004-2009 D-Link Systems, Inc.