D-LINK SYSTEMS, INC. | WIRELESS AP : HELP / Status

# Help MENU

Status

Device Info
This page displays the current information of the DAP-1350. The page will show the firmware currently loaded, wired and wireless settings applied on the unit.
LAN (Local Area Network) - This displays the MAC Address, the IP Address, Subnet Mask and Default Gateway of the Ethernet LAN interface and whether or not the AP's built-in DHCP server is Enabled or Disabled.
WIRELESS LAN - This displays the MAC Address, Wireless Network Name (SSID), Wireless Channel and Wireless Security Type of the Wireless LAN interface.

Log
The DAP-1350 keeps a running log of events and activities occurring on it at all times. The log will display up to 200 recent logs. Newer log activities will overwrite the older logs. You can save the log files or have them emailed to you by clicking on the Log Settings button. This is recommended as the logs are cleared every time the AP is rebooted.
First Page - Click this button to go to the first page of the log.
Last Page - Click this button to go to the last page of the log.
Previous - Moves back one log page.
Next - Moves forward one log page.
Clear - Clears the logs completely.
Log Settings - If you would like to see the AP's logs,please enable the syslog.

Statistics Displays data packet statistics of both transmitted frame and received frame for the DAP-1350 network. Refresh - Click this button to update the counters.

Copyright © 2009 D-Link Corporation/D-Link System, Inc.