D-LINK SYSTEMS, INC | WIRELESS ROUTER | TOOLS

Product Page: DIR-451 | Hardware Version: A1 | Firmware Version: v1.03_NA

| Setup | Advanced | Tools | Status | Support

- Admin
- Time
- System
- Firmware
- DDNS
- SYSTEM CHECK
- SCHEDULES
- Log settings
- Syslog
- Email Settings
- Routing

# Dynamic DNS :

Dynamic DNS (Domain Name Service) is a method of keeping a domain name linked to a changing (dynamic) IP address. With most Cable and DSL connections, you are assigned a dynamic IP address and that address is used only for the duration of that specific connection.

With the DIR-451, you can setup your DDNS service and the DIR-451 will automatically update your DDNS server every time it receives a new WAN IP address.

## ddns Settings :

Enable DDNS : |
Server Address : |
Host Name : |
Username : |
Password : |

Helpful Hints.. DDNS: In order to use this feature you must first have a DDNS account from one of the providers in the drop down menu.

Copyright © 2004-2008 D-Link Systems, Inc.