D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Setup / WAN

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

- Internet Settings
- Wireless Settings
- Network Settings
- USB Settings
- Logout

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## WAN

Use this section to configure your Internet Connection type. There are several connection types to choose from: Static IP, DHCP, PPPoE, PPTP, L2TP , and Usb3g. If you are unsure of your connection method, please contact your Internet Service Provider.

Note : If using the PPPoE option, you will need to remove or disable any PPPoE client software on your computers.

Note: Only Administrator has access to some of these functionalities.

### Internet Connection Type

Choose the mode to be used by the router to connect to the Internet.

My Internet Connection is :

### Usb3g Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

ISP Name :

APN : Auto

Manual

Dial Number :

PIN : (Option)

Verify PIN : (Option)

Auth Protocol :

Username : (Option)

Password : (Option)

Verify Password : (Option)

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

Keep-alive Interval : (seconds)

Keep-alive Server1 : (Option)

Keep-alive Server2 : (Option)

Helpful Hints...

When configuring the router to access the Internet, be sure to choose the correct Internet Connection Type from the drop down menu. If you are unsure of which option to choose, contact your Internet Service Provider (ISP).

If you are having trouble accessing the Internet through the router, double check any settings you have entered on this page and verify them with your ISP if needed.

For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs.

If you are having trouble receiving multicast streams from the Internet, make sure the Multicast Streams option is enabled.

More...

Copyright © 2009 D-Link Corporation/D-Link System, Inc.