> > Add Network Traffic Class Rule

> > The screen creates a traffic class rule to classify the upstream traffic, assign queuing priority and optionally overwrite the IP header TOS byte. A rule consists of a class name and at least one condition below. All of the specified conditions in this classification rule must be satisfied for the rule to take effect. Click 'Apply' to save and activate the rule.

> > Traffic Class Name:

> > Enable Differentiated Service Configuration

> > Assign ATM Priority and/or IP Precedence and/or Type Of Service for the class
> > If non-blank value is selected for 'Mark IP Precedence' and/or 'Mark IP Type Of Service', the correcponding TOS byte in the IP header of the upstream packet is overwritten by the selected value.
> > Note: If Differentiated Service Configuration checkbox is selected, you will only need to assign ATM priority. IP Precedence will not be used for classification. IP TOS byte will be used for DSCP mark.

> > Assign ATM Transmit Priority: |
> > Assign Differentiated Services Code Point (DSCP) Mark: |
> > Mark IP Precedence: |
> > Mark IP Type Of Service: |
> > Mark 802.1p if 802.1q is enabled on WAN: |
> > Specify Traffic Classification Rules
> > Enter the following conditions either for IP level, SET-1, or for IEEE 802.1p, SET-2.
> > SET-1
> > Physical LAN Port: |
> > Protocol: |
> > Source IP Address: |
> > Source Subnet Mask: |
> > UDP/TCP Source Port (port or port:port): |
> > Destination IP Address: |
> > Destination Subnet Mask: |
> > UDP/TCP Destination Port (port or port:port): |
> > Source MAC Address: |
> > Source MAC Mask: |
> > Destination MAC Address: |
> > Destination MAC Mask: |
> > SET-2
> > 802.1p Priority: |