dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- User Management
- RAID
- Backup and Restore
- Firmware Update
- Logout

#
HARD DRIVE CONFIGURATION

Change the hard drive configuration or format the newly inserted drive.If you are not first time to configure your hard disk on the NVR, please refer to current disk status from STATUS > Device Info > HARD DRIVE INFORMATION before you make any changes.

##
RAID CONFIGURATION

Helpful Hints..
To see information on the current hard disk configuration, go to the STATUS page.
The NVR supports four different disk configuration types: Standard, where each drive is a unique volume,JBOD, which combines both drives in a linear fashion to create one volume, as well as RAID 0 and RAID 1.

RAID, short for Redundant Array of Independent Disks, is a combination of two or more disks with the aim of providing fault tolerance and improving performance. There are several different levels of RAID, with each providing a different method of sharing or distributing data amongst the drives. The NVR supports RAID levels 0 and 1.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.