> > Wireless -- Advanced

> > This page allows you to configure advanced features of the wireless LAN interface. You can select a particular channel on which to operate, force the transmission rate to a particular speed, set the fragmentation threshold, set the RTS threshold, set the wakeup interval for clients in power-save mode, set the beacon interval for the access point, set XPress mode and set whether short or long preambles are used.
> > Click "Apply" to configure the advanced wireless options.

> > AP Isolation: |
> > Band: |
> > Channel: |  | Current: 11
> > Auto Channel Timer(min) |

> > 802.11n/EWC: |

> > Bandwidth: |  | Current: MHz
> > Control Sideband: |  | Current: N/A
> > 802.11n Rate: |
> > 802.11n Protection: |

> > 54g™ Rate: |
> > Multicast Rate: |
> > Basic Rate: |
> > Fragmentation Threshold: |
> > RTS Threshold: |
> > DTIM Interval: |
> > Beacon Interval: |
> > XPress™ Technology: |

> > 54g™ Mode: |
> > 54g™ Protection: |

> > Regulatory Mode: |
> > Pre-Network Radar Check: |
> > In-Network Radar Check: |
> > TPC Mitigation(db): |

> > Afterburner Technology: |  | Disable WMM(Quality of Service) and set Fragmentation to 2346 for selection

> > Preamble Type: |

> > Transmit Power: |