D-LINK SYSTEMS, INC. | WIRELESS AP : Setup / Wireless Setup

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

- Setup Wizard
- Wireless Setup
- Lan Setup
- Logout

## Wireless Connection

Use this section to configure the wireless settings for your D-Link Access Point. Please note that changes made on this section will also need to be duplicated to your wireless clients and PC.

To protect your privacy you can configure wireless security features. This device supports three wireless security modes including: WEP or WPA and WPA2.

### Wireless Network Settings

Enable Wireless :

Wireless Mode : Access Point

Wireless Network Name : (Also called the SSID)

Enable Auto Channel Scan :

Wireless Channel :

802.11 Mode :

Channel Width :

Transmission Rate :

Enable Hidden Wireless : (Also called Disable SSID Broadcast)

### Wireless Security Mode

Security Mode :

### WEP

WEP is the wireless encryption standard. To use it you must enter the same key(s) into the router and the wireless stations. For 64 bit keys you must enter 10 hex digits into each key box. For 128 bit keys you must enter 26 hex digits into each key box. A hex digit is either a number from 0 to 9 or a letter from A to F. For the most secure use of WEP set the authentication type to "Shared Key" when WEP is enabled.

You may also enter any text string into a WEP key box, in which case it will be converted into a hexadecimal key using the ASCII values of the characters. A maximum of 5 text characters can be entered for 64 bit keys, and a maximum of 13 characters for 128 bit keys.

Authentication :

WEP Key Length :

Key Format :

Default WEP Key :

WEP Key 1 :

WEP Key 2 :

WEP Key 3 :

WEP Key 4 :

### WPA

WPA requires stations to use high grade encryption and authentication.

### WPA2

WPA2 requires stations to use high grade encryption and authentication.

### WPA2-Auto

WPA2-Auto requires stations to use high grade encryption and authentication.

Cipher Type :

PSK / EAP :

Passphrase :

Confirmed Passphrase :

RADIUS Server 1 : IP

Port

Shared Secret

RADIUS Server 2 : IP

Port

Shared Secret

### WIFI Protected Setup (also called wcn 2.0 in windows vista)

Enable :

Current PIN:

Wi-Fi Protected Status : Enabled/Configured

Helpful Hints...

Wireless Network Name:
Changing your Wireless Network Name is the first step in securing your wireless network. We recommend that you change it to a familiar name that does not contain any personal information.

Hidden Wireless:
Enabling Hidden Mode is another way to secure your network. With this option enabled, no wireless clients will be able to see your wireless network when they perform scan to see what's available. In order for your wireless devices to connect to your AP, you will need to manually enter the Wireless Network Name on each device.

Security Keys:
If you have enabled Wireless Security, make sure you write down WEP Key or Passphrase that you have configured. You will need to enter this information on any wireless device that you connect to your wireless network.

Wi-Fi Protected Setup (Also called WCN 2.0 in Windows Vista):
Wi-Fi Protected Setup provides a more intuitive way of setting up wireless security between the AP and the wireless client. Make sure the wireless card supports such feature or uses a certified Windows Vista driver in order to take advantage of this feature.

Copyright © 2009 D-Link Corporation/D-Link System, Inc.