Device Info
DHCP Clients
Log
Statistics
ADSL
Logout

Traffic Statistics
Traffic Statistics display Receive and Transmit packets passing through the DSL-G604T.
Choose an interface to view your network status:
Ethernet | Display Receive and Transmit packages through Ethernet
ADSL | Display Receive and Transmit packages through ADSL
Wireless | Display Receive and Transmit packages through wireless connection
Transmit
| Good Tx Frames | 4030 |
| Good Tx Broadcast Frames | 5 |
| Good Tx Multicast Frames | 0 |
| Tx Total Bytes | 2640125 |
| Collisions | 0 |
| Error Frames | 0 |
| Carrier Sense Errors | 0 |
Receive
| Good Rx Frames | 3070 |
| Good Rx Broadcast Frames | 187 |
| Good Tx Multicast Frames | 25 |
| Rx Total Bytes | 375872 |
| CRC Errors | 0 |
| Undersized Frames | 0 |
| Overruns | 0 |