D-LINK SYSTEMS, INC. | WIRELESS CLIENT : Advanced / Advanced Wireless

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

## Advanced Wireless

These options are for users that wish to change the behaviour of their 802.11n wireless radio from the standard setting. D-link does not recommend changing these settings from the factory default. Incorrect settings may impair the performance of your wireless radio. The default settings should provide the best wireless radio performance in most environments.

Note: Only Administrator has access to some of these functionalities.

### Advanced Wireless Settings

Transmit Power :

RTS Threshold : (1..2347)

Fragmentation Threshold : (256..2346)

Short GI :

Helpful Hints...

Advanced Wireless:
It is recommended that you leave these options at their default values. Adjusting them could negatively impact the performance of your wireless network.
The options on this page should be changed by advanced users or if you are instructed to by one of our support personnel, as they can negatively affect the performance of your Access Point if configured improperly.

Transmit Power:
You can lower the output power of the DAP-1350 by selecting lower percentage Transmit Power values from the drop down. Your choices are: 100%, 50%, 25%, and 12.5%.

Copyright © 2009 D-Link Corporation/D-Link System, Inc.