D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / Advanced Wireless

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Advanced Wireless

If you are not familiar with these Advanced Wireless settings, please read the help section before attempting to modify these settings.

Note: Only Administrator has access to some of these functionalities.

### Advanced Wireless Settings

Transmit Power :

Beacon Period : (20..1024)

DTIM Interval : (1..255)

RTS Threshold : (1..2347)

Fragmentation Threshold : (256..2346)

WMM Enable :

Short GI :

IGMP Snooping :

WLAN Partition :

Helpful Hints...

It is recommended that you leave these parameters at their default values. Adjusting them could limit the performance of your wireless network.

Enabling WMM can help control latency and jitter when transmitting multimedia content over a wireless connection.

More...

Copyright © 2009 D-Link Corporation/D-Link System, Inc.