D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-330 | Firmware Version: 1.12

| Setup | Advanced | Maintenance | Status | Help

- Internet
- Wireless settings
- Network settings
- VPN Settings

# Network Settings :

Use this section to configure the internal network settings of your router and also to configure the built-in DHCP Server to assign IP addresses to the computers on your network. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

## Router Settings :

Use this section to configure the internal network settings of your router. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

Router IP Address : |
Default Subnet Mask : |
Local Domain Name : |
Enable DNS Relay : |

## DHCP Server Settings :

Use this section to configure the built-in DHCP Server to assign IP addresses to the computers on your network.

Enable DHCP Server : |
DHCP IP Address Range : | to (addresses within the LAN subnet)
DHCP Lease Time : | (minutes)

## Dynamic DHCP Client List :

Host Name | IP Address | MAC Address | Expired Time |
End User | 192.168.0.112 | 00:04:23:2c:44:9f | Sat Mar 2 00:00:41 2002

## 50 - DHCP Reservations List :

Remaining number of DHCP Reservations that can be configured: 50 | More...
Remaining number of DHCP Reservations that can be configured: 50 | Back...

| Computer Name | IP Address | MAC Address |
1. |  | 192 . 168 . 0 . |  |
2. |  | 192 . 168 . 0 . |  |
3. |  | 192 . 168 . 0 . |  |
4. |  | 192 . 168 . 0 . |  |
5. |  | 192 . 168 . 0 . |  |
6. |  | 192 . 168 . 0 . |  |
7. |  | 192 . 168 . 0 . |  |
8. |  | 192 . 168 . 0 . |  |
9. |  | 192 . 168 . 0 . |  |
10. |  | 192 . 168 . 0 . |  |
11. |  | 192 . 168 . 0 . |  |
12. |  | 192 . 168 . 0 . |  |
13. |  | 192 . 168 . 0 . |  |
14. |  | 192 . 168 . 0 . |  |
15. |  | 192 . 168 . 0 . |  |
16. |  | 192 . 168 . 0 . |  |
17. |  | 192 . 168 . 0 . |  |
18. |  | 192 . 168 . 0 . |  |
19. |  | 192 . 168 . 0 . |  |
20. |  | 192 . 168 . 0 . |  |
21. |  | 192 . 168 . 0 . |  |
22. |  | 192 . 168 . 0 . |  |
23. |  | 192 . 168 . 0 . |  |
24. |  | 192 . 168 . 0 . |  |
25. |  | 192 . 168 . 0 . |  |

26. |  | 192 . 168 . 0 . |  |
27. |  | 192 . 168 . 0 . |  |
28. |  | 192 . 168 . 0 . |  |
29. |  | 192 . 168 . 0 . |  |
30. |  | 192 . 168 . 0 . |  |
31. |  | 192 . 168 . 0 . |  |
32. |  | 192 . 168 . 0 . |  |
33. |  | 192 . 168 . 0 . |  |
34. |  | 192 . 168 . 0 . |  |
35. |  | 192 . 168 . 0 . |  |
36. |  | 192 . 168 . 0 . |  |
37. |  | 192 . 168 . 0 . |  |
38. |  | 192 . 168 . 0 . |  |
39. |  | 192 . 168 . 0 . |  |
40. |  | 192 . 168 . 0 . |  |
41. |  | 192 . 168 . 0 . |  |
42. |  | 192 . 168 . 0 . |  |
43. |  | 192 . 168 . 0 . |  |
44. |  | 192 . 168 . 0 . |  |
45. |  | 192 . 168 . 0 . |  |
46. |  | 192 . 168 . 0 . |  |
47. |  | 192 . 168 . 0 . |  |
48. |  | 192 . 168 . 0 . |  |
49. |  | 192 . 168 . 0 . |  |
50. |  | 192 . 168 . 0 . |  |

More...
Back...

Helpful Hints.. If you already have a DHCP server on your network or are using static IP addresses on all the devices on your network, uncheck Enable DHCP Server to disable this feature. In order to ensure that devices on your network are always assigned the same IP address, add a DHCP Reservation for each device.

Copyright © 2004-2005 D-Link Systems, Inc.