DNS-343

Maintenance
Admin Password The administrator's password is changed here. Enter in the current password first and then the new password. Type in the new password again and click 'Save Settings' to put the change into effect.

System
Restart Click 'Restart' to reboot the DNS-343.
Defaults
Click 'Restore' to reset the DNS-343 to factory default settings. Use the restore feature only if necessary as this will erase all previously saved settings on the unit. This process will not harm or change any data on the internal drives.
Shutdown
Power off the unit.
Configuration Settings
Save configuration settings by pressing the 'Save' button and choosing a location for the configuration file to save to.
Load configuration settings by pressing the 'Browse' button to find the configuration file, then pressing the 'Load' button to load the file.
Idle Time
Enter a value for the System Inactivity Timer. If the administrator is idle for longer than the specified time, he will be logged out of the configuration area.
Enter a value for the Download Schedule Inactivity Timer. If a user is idle for longer than the specified time, he will be logged out of the Schedule Download area.

Click 'Apply' when finished.

Firmware You can upgrade the firmware of the device from this page. The firmware you want to use must be saved on the local hard drive of the computer you are working from. Click on 'Browse' to search the local hard drive for the firmware to be used for the update. Click 'Apply' to begin the upgrade. Please check the D-Link support site for firmware updates at D-Link Support Page.

E-Mail Alerts
Login Method
Select 'Account' if your SMTP server requires authentication. Select 'anonymous' if it does not.
User Name
If 'Account' is selected, enter the user name of your e-mail account.
Password
If 'Account' is selected, enter the password for your e-mail account.
SMTP Server
Enter the SMTP Server address. This will be your outgoing mail server address. If you're not sure what this is, contact the company that provides e-mail services for you.
Sender E-Mail
Enter the Sender's e-mail address. This is the address that the e-mail alerts will appear to be coming from.
Receiver E-Mail
Enter the Receiver's e-mail address. This is the address you want the e-mail alerts sent to.
Alert Types
Select the information you want e-mailed to the above address. The space status can be sent in intervals, while the other items will only be sent when necessary.
Click 'Save Settings' when finished.

Power Management
This section allows you to enable or disable the Hard Drive Hibernation and Power Recovery function.
Hard Drive Hibernation
Select the amount of time before the hard drives will shut down. Remember that the device will stay powered on. Only the hard drives will lose power. They will re-gain power immediately after attempting to access them.
Power Recovery
If enabled, in the event of a power failure the DNS-343 will turn on and resume operation once power has been restored.
Click 'Save Settings' when finished.

Dynamic DNS
Enable this option only if you have purchased your own domain name and registered with a dynamic DNS service provider. The following parameters are displayed when the option is enabled.

Server Address
Select a dynamic DNS service provider from the pull-down list.
Host Name
Enter your host name, fully qualified; for example: myhost.mydomain.net.
Username or Key
Enter the username or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Password or Key
Enter the password or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Verify Password or Key
Re-type the password or key provided by your service provider. If the Dynamic DNS provider supplies only a key, enter that key in all three fields.
Timeout
The time between periodic updates to the Dynamic DNS, if your dynamic IP address has not changed. The timeout period is entered in hours.
Status
Displays the current status of connection to Dynamic DNS server.

OLED Display Sleep When the OLED is idle, it will go into sleep mode after a pre-configured time ranging from 10 to 30 seconds and up to 1, 5, 10 and 15 minutes.
Scan Disk Scan Disk Scan disk and list errors if exist.