D-Link Corporation. | WIRELESS INTERNET CAMERA | SETUP | MAIL

Product: DCS-920 |  | Firmware Version: 1.00

| Live Video | Setup | Maintenance | Status | Help

Wizard
Network Setup
Wireless Setup
Dynamic DNS
Image Setup
Video
Mail
FTP
Time and Date
Logout

# Mail

This section allows you to setup and configure the email notification settings for your camera. If your details change or you are experiencing issues with alert notifications, you may need to modify these settings.

## E-mail Account

SMTP Server Address |
Sender E-mail Address |
Receiver E-mail Address |
User Name |
Password |

## Time Schedule

| Enable emailing images to email account

Always

| Schedule
| Day | Mon Tue Wed Thu Fri Sat Sun
| Time Period | Start : (Example : 06:30:00) Stop : (Example : 22:30:00)

Interval Seconds

## Test E-mail Account

| A test email will be sent to the e-mail account listed above. |

Helpful Hints..
SMTP Server Address:
This is the domain name or IP address of your external email server.
Sender E-mail Address:
This is the email address of the person sending the camera snapshots.
Receiver E-mail Address:
This is the email address of recipient for the SMTP server.
User Name:
The user name of your email account.
Password:
The password of your email account.
Enable emailing images to email account:
Select Always to enable camera sending images to the recipient's email account.
Select Schedule if you would like to specify the time and day when the camera starts and stops sending images to the recipient's email account. The interval of the snapshot can also be configured from 1 to 65535 seconds.

Copyright (C) 2007-2008 D-Link Corporation.