> > TR-069 client - Configuration

> > WAN Management Protocol (TR-069) allows a Auto-Configuration Server (ACS) to perform auto-configuration, provision, collection, and diagnostics to this device.
> > Select the desired values and click "Apply" to configure the TR-069 client options.

> > Inform | Disable | Enable

> > Inform Interval: |
> > ACS URL: |
> > ACS User Name: |
> > ACS Password: |
> > Connection Request User Name: |
> > Connection Request Password: |