dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup>
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup
- Logout

# LIVE AND PLAYBACK SETUP

For live viewing and playback over the internet, you need to dedicate a port for the streaming server.

## LIVE STREAMING SERVER

Port |
Maximum Connections |

## PLAYBACK SERVER

Port |
Maximum Users |

## ALLOWED/BLOCKED LIST

Allowed List | Enable
Blocked List | Enable

IP Range

to

Helpful Hints..

If NVR is placed behind a NAT router, open the port on the router for the Live and Playback streaming server. The following list briefly describes the Live and Playback Setup menu items:
Maximum Connections: The maximum number of remote connections is 32.
Maximum Users: The maximum number of users for the playback server is 8.
Allowed List: Allows only certain IP Addresses to log in for live view and playback
Blocked List: IP addresses in this list will always be blocked
Note
If the maximum number of connections is 16 and if a user connects to 4 cameras, the number of connected users is 4 and not 16.

Copyright © 2008 D-Link Corporation/D-Link System, Inc.