D-Link Print Server - Advanced Wireless

Product Page: DPR-1260 | Firmware Version: 1.24

| Status | Scan | Advanced | Setup | Help

- Printing
- Wireless
- System

# Advanced Wireless

If you are not familiar with these Advanced Wireless settings, please read the help section before attempting to modify these settings.

## Wireless Settings

Fragmentation threshold | (256..65535)
RTS threshold | (1..65535)
Burst time | (0..65535)
Beacon period | (1..65535)

802.11d |

Helpful Hints..
Wireless Settings:
Fragmentation Threshold - Transmitted wireless packets larger than this size will be fragmented to maintain performance in noisy wireless networks. The valid range is 256..65535. Values larger than about 1560 will prevent fragmentation from taking place.
RTS threshold - Transmitted wireless packets larger than this size will use the RTS/CTS protocol to (a) maintain performance in noisy wireless networks and (b) prevent hidden nodes from degrading performance. The valid range is 1..65535. Values larger than about 1560 will prevent RTS/CTS from taking place.
Burst time - Set the time duration here for transmission burst mode, in microseconds. The valid range is 0..65535 with 0 to disable bursting. Burst mode can increase data throughput by occupying the channel for an extended duration. Typical values are in the range of several mili-seconds (ie. 3000).
Beacon period - In adhoc mode beacons are sent out periodically. This is the number of milliseconds between each beacon. The valid range is 1..65535.

Copyright © 2006 D-Link Systems, Inc.