D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-330 | Firmware Version: 1.12

| Setup | Advanced | Maintenance | Status | Help

- Internet
- Wireless Settings
- Network Settings
- VPN Settings

# Wireless Network :

Use this section to configure the wireless settings for your D-Link router. Please note that changes made on this section may also need to be duplicated on your wireless client.
To protect your privacy you can configure wireless security features. This decive supports three wireless security modes including: WEP, WPA and WPA2.

## WI-FI PROTECTED SETUP (ALSO CALLED WCN 2.0 IN WINDOWS VISTA) :

Enable : |
Current PIN : | 12345670
Wi-Fi Protected Setup Status: | Enabled / Not Configured

## Wireless Network Settings :

Enable Wireless : |
Wireless Network Name : | (Also called the SSID)
Wireless Channel : |
Enable Auto Channel Selection : |
802.11 Mode : |
Enable Hidden Wireless : | (Also called the SSID Broadcast)

## Wireless Security Mode :

You can configure the wireless security features of your router to protect your privacy. This device supports three different wireless security modes: WEP, WPA-Personal and WPA-Enterprise. WEP is the original wireless encryption standard. WPA provides a higher level of security. WPA-Personal does not require an authentication server. WPA-Enterprise requires an external RADIUS server.

Security Mode : |

## WEP :

WEP is the wireless encryption standard. To use it you must enter the same key(s) into the router and the wireless stations. For 64 bit keys you must enter 10 hex digits into each key box. For 128 bit keys you must enter 26 hex digits into each key box. A hex digit is either a number from 0 to 9 or a letter from A to F. For the most secure use of WEP set the authentication type to "Open System" when WEP is enabled.

You may also enter any text string into a WEP key box, in which case it will be converted into a hexadecimal key using the ASCII values of the characters. A maximum of 5 text characters can be entered for 64 bit keys, and a maximum of 13 characters for 128 bit keys.

Authentication : |
WEP Encryption : |
Default WEP Key : |
WEP Key : | (5 ASCII or 10 HEX)
WEP Key : | (13 ASCII or 26 HEX)

## WPA Only

WPA Only requires stations to use high grade encryption and authentication.

## WPA2 Only

WPA2 Only requires stations to use high grade encryption and authentication.

## WPA/WPA2

WPA/WPA2 requires stations to use high grade encryption and authentication.

Cipher Type : | undefined
PSK / EAP : |
Network Key : | (8~63 ASCII or 64 HEX)

802.1X
RADIUS Server | IP Address | :
RADIUS Server | Port | :
RADIUS Server | Shared Secret | :

Helpful Hints..

Wi-Fi Protected Setup provides a more intuitive way of setting up wireless security between the router and the wireless client. Make sure the wireless card supports such feature or uses a certified Windows Vista driver in order to take advantage of this feature.

Changing your Wireless Network Name is the first step in securing your wireless network. We recommend that you change it to a familiar name that does not contain any personal information.

Enabling Hidden Mode is another way to secure your network. With this option enabled, no wireless clients will be able to see your wireless network when they perform scan to see what's available. In order for your wireless devices to connect to your router, you will need to manually enter the Wireless Network Name on each device.

If you have enabled Wireless Security, make sure you write down WEP Key or Passphrase that you have configured. You will need to enter this information on any wireless device that you connect to your wireless network.

The DIR-330 only supports mandatory cipher type in WPA and WPA2. They are: WPA only supports TKIP, WPA2 only supports AES, WPS doesn't support WEP encrpytion.

Copyright © 2004-2005 D-Link Systems, Inc.