D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-330 | Firmware Version: 1.12

| Setup | Advanced | Maintenance | Status | Help

- Device Info
- Log
- Statistics
- Active Session
- Wireless Clients
- LAN Clients
- Routing
- VPN

# Device InfoRMATION :

All of your Internet and network connection details are displayed on this page. The firmware version is listed below.

Firmware Version: 1.12

## LAN :

MAC Address : | 00:1C:F0:F0:68:DC
IP Address : | 192.168.0.1
Subnet Mask : | 255.255.255.0
DHCP Server : | Enabled

## Wan :

MAC Address : | 00:1C:F0:F0:68:DD
Connection : | DHCP Client Connected
IP Address : | 172.16.100.193
Subnet Mask : | 255.255.255.0
Default Gateway : | 172.16.100.1
DNS : | 4.2.2.2 4.2.2.3

## Wan Physical:

MAC Address : | 00:1C:F0:F0:68:DD
Connection : | fixed IP
IP Address : | 0.0.0.0
Subnet Mask : | 0.0.0.0
Default Gateway : | 0.0.0.0
DNS : | 4.2.2.2 4.2.2.3

## Wan Physical:

MAC Address : | 00:1C:F0:F0:68:DD
Connection : | fixed IP
IP Address : | 172.16.100.193
Subnet Mask : | 255.255.255.0
Default Gateway : | 172.16.100.1
DNS : | 4.2.2.2 4.2.2.3

## WIRELESS :

SSID : | DIR-330
Channel : | 6
Encryption : | WPA-PSK

Helpful Hints.. All of your Internet and network connection details are displayed on the Device Info page. The firmware version is also displayed here.

Copyright © 2004-2005 D-Link Systems, Inc.