> > Routing -- RIP Configuration

> > To activate RIP for the device, select the 'Enabled' radio button for Global RIP Mode. To configure an individual interface, select the desired RIP version and operation,followed by placing a check in the 'Enabled' checkbox for the interface. Click the 'Apply' button to save the configuration, and to start or stop RIP based on the Global RIP mode selected.

> > Global RIP Mode | Disabled | Enabled

> > Interface | VPI/VCI | Version | Operation | Enabled
> > br0 | (LAN) |  |  |