dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Menu
- Live Video
- Playback
- Setup
- Maintenance
- Status
- Logout

#
HELP MENU

- Live Video

##
LIVE VIDEO

Setup Live View
1. Open Internet Explorer and login the NVR.
2. Search and setup the cameras.
3. Click the LIVE VIDEO button on the top of the page.
4. Select a camera(s) from the camera list on the right and then drag it to where you wish the image to be displayed.
5. User can drag the change the video display position again by drag it to another position.
6. Specified video will be marked with green line. Right click on the video can Toggle to Full Screen. Press ESC button on the keyboard can return to normal display.
7. If the camera supports audio, user can check Enable Audio from the right click menu and listen to live audio of this channel.
8. If the camera supports PTZ, user can control the specify camera from the PTZ panel. Or user can check Enable Move from the right click menu click on the video to control the PTZ function directly. Please note when Enable Move is checked, the video will mark with red line. It means user can not change to any other cameras unless this function unselected.
Single / Quad split Screen
User can select to view single camera or 4 cameras at a time.
Snapshot
Select the snapshot function to capture a specific video image immediately.
Full Screen
Select to display the video with full screen. Press ESC button on the keyboard can return to normal display.
PTZ Camera Control
You may control the camera view by utilizing the PTZ camera control panel to adjust the camera's view. This is only available with cameras that support PTZ function.
Zoom
Click the + or - button to zoom in or zoom out the view. This is only available with cameras that support optical zoom function.
Preset
Click the Set button to set the preset position of PTZ camera. User can give the specify position a name and store it into preset position list. Click the Go button to go to the preset position. This is only available with cameras that support preset function.
Digital Zoom
Click the icon to digital zoom in or digital zoom out the view. Every camera can use this function.
Play / Stop / Drop
Select a camera/ video and click this button to play/stop/disconnect a particular channel.
Information Display Window
Display video information including camera name, video status, and bit rate for a selected channel.
Remote I/O
Utilize I/O device function remotely. User can remotely adjust the Output Pins by turning it on or off.

Copyright © 2008 D-Link Corporation/D-Link Systems, Inc.