D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Disk Management
- Users/Groups
- Storage Access
- FTP Server
- UPnP AV Server
- iTunes Server
- BT Download Manager

# Ftp Server Settings

Assign permissions for users and groups that will access the FTP server over the Internet.

## Ftp Server Settings

Category | User Group
Group |
User | All accounts
Folder | root
Permission |

Enable FTP | Enable Disable
Mode | LAN Internet/WAN LAN + Internet/WAN
Max. User |
Idle Time | Idle Time
Port | ( 1~65535,Default:21)
Flow Control | Unlimited x 10 KBs |
Client Language |  |

## Ftp Access List

:R/W : Read/Write :Read Only :Modify settings :Delete
Path | User/Group | R/W |  |

## Ftp Server Status

| Status | Stopped
| Mode | LAN
| Port | 21
| Max. User | 10
| Flow Control | Unlimited
| Idle Time | 5
| Client Language | Western European

Helpful Hints..

• If your DIR-685 is connected to a router, you will need to forward port 21 (in the router configuration) to the IP address of the DIR-685. From the outside world, remember to access this FTP server by using the WAN address of your router.

More...

Copyright © 2004-2007 D-Link Systems, Inc.