D-Link Corporation. | WIRELESS INTERNET CAMERA | SETUP | WIRELESS SETUP

Product: DCS-920 |  | Firmware Version: 1.00

| Live Video | Setup | Maintenance | Status | Help

Wizard
Network Setup
Wireless Setup
Dynamic DNS
Image Setup
Video
Mail
FTP
Time and Date
Logout

# Wireless Setup

In this section, you can setup and configure the wireless settings on your camera.

## wireless settings

Enable Disable

## basic wireless settings

SSID |
Channel |
Connection Mode | Infrastructure Ad-Hoc

## Wireless Security Mode

Security Mode | None WEP WPA-PSK / WPA2-PSK

## WEP Settings

Authentication | Open System Shared Key Both
Encryption Mode |
Key Format |
Default Key |
Key1 |
Key2 |
Key3 |
Key4 |

## WPA-PSK / WPA2-PSK Settings

Pre-Shared Key | (8-63 ASCII or 64 HEX characters)

Helpful Hints..
You may enable the wireless setting on your camera and connect to a wireless network by entering the SSID (unique name of your wireless network), or click the Site Survey button to select an available wireless network. Then you may choose a channel number. When there is interference from the wireless networks that overlap with one another, you may change the channel to obtain maximum performance from your connection.
There are two connection modes. Infrastructure is a wireless connection using an access point as a transmission point of all wireless devices. Ad-Hoc is a wireless connection used without an access point, which connects the PC directly to the DCS-920.
WPS - The WPS (Wi-Fi Protected Setup) wizard will allow you to easily connect the camera to your wireless network.
For security there are three choices of wireless encryption , None, WEP, and WPA-PSK / WPA2-PSK. Select the same encryption method that is being used by your wireless device/ router. If you have selected WPA-PSK or WPA2-PSK setting, you may need to enter the appropriate Pre-Shared Key in order to connect to the wireless network.

Copyright (C) 2007-2008 D-Link Corporation.