> > WAN
> > Connection Type
> > Select the type of network protocol and encapsulation mode over the ATM PVC that your ISP has instructed you to use. Note that 802.1q VLAN tagging is only available for PPPoE, MER and Bridging.

> > PPP over ATM (PPPoA)
> > PPP over Ethernet (PPPoE)
> > MAC Encapsulation Routing (MER)
> > IP over ATM (IPoA)
> > Bridging

> > Encapsulation Mode

> > Enable 802.1q |

> > VLAN ID[0-4095]: |